Proposal to amend GRE/2020/05.

1. Proposal

*Add a new paragraph 4.5.6.,* amend to read:

"4.5.6. On request of the applicant, the internal structure of the optical components and/or the texture of the outer lens inside of the apparent surface of a lamp (function) may incorporate only one manufacturer logo build by tranparent or non transparent components provided that all requirements for the specific function of this Regulation are fulfilled and in addition the following conditions:

(a) Irrespective of the marking requirements in paragraph 3.3., only the logo of the brand name of the vehicle manufacturer or the body manufacturer is allowed. This shall be confirmed by the applicant by a statement (see paragraph 3.1.2.2. (e)).

(b) Size: the enclosed light emitting surface of the logo (incorporating tranparent or non transparent components of the logo) of such a lamp in the direction of the reference axis shall not exceed 100 cm2.

(c) Symmetry: notwithstanding the requirements of paragraph 5.5.2. of UN Regulation No. 48, the logo **(incorporating transparent or non-transparent components of the logo)** light emitting surface does not have to be symmetrical by itself.”

(d) Stop lamps, direction indicator lamps, **and** reversing lamps **~~and manoeuvring lamps~~** shall not incorporate a logo..”

1. **Justification:**

1. It is important that the complete logo (transparent and non-transparent) has not to be symmetrical.