|  |  |
| --- | --- |
|  | E/ECE/324/Rev.1/Add.97/Rev.3/Amend.5−E/ECE/TRANS/505/Rev.1/Add.97/Rev.3/Amend.5 |
|  |  | 9 November 2015 |

 Agreement

 Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

 Addendum 97 – Regulation No. 98

 Revision 3 - Amendment 5

Supplement 6 to the 01 series of amendments – Date of entry into force: 8 October 2015

 Uniform provisions concerning the approval of motor vehicle headlamps equipped with gas-discharge light sources

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2015/27.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Annex 4,*

*Paragraph 1.2.1.1.*, amend to read:

"1.2.1.1. Test mixture

1.2.1.1.1. For headlamp with the outside lens in glass:

The mixture of water and a polluting agent to be applied to the headlamp shall be composed of:

9 parts by weight of silica sand with a particle size of 0-100 μm,

1 part by weight of vegetal carbon dust produced from beech wood with a particle size of 0-100 μm,

0.2 parts by weight of NaCMC3, and

5 parts by weight of sodium chloride (pure at 99 per cent),

an appropriate quantity of distilled water, with a conductivity
of ≤ 1 µS/m.

The mixture must not be more than 14 days old.

1.2.1.1.2. For headlamp with outside lens in plastic material:

The mixture of water and polluting agent to be applied to the headlamp shall be composed of:

9 parts by weight of silica sand with a particle size of 0-100 μm,

1 part by weight of vegetal carbon dust produced from beech wood with a particle size of 0-100 μm,

0.2 part by weight of NaCMC3,

5 parts by weight of sodium chloride (pure at 99 per cent),

13 parts by weight of distilled water with a conductivity of ≤ 1 µS/m, and

2 ± 1 parts by weight of surface-actant.4

The mixture must not be more than 14 days old."

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)