|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.1/Add.40/Rev.2/Amend.5−E/ECE/TRANS/505/Rev.1/Add.40/Rev.2/Amend.5 | |
|  |  | 22 February 2017 |

Agreement

Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

Addendum 40 – Regulation No. 41

Revision 2 - Amendment 5

Supplement 5 to the 04 series of amendments – Date of entry into force: 9 February 2017

Uniform provisions concerning the approval of motor cycles with regard to noise

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2016/46.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Annex 5,*

*Paragraph 1*., amend to read:

"1. Fibrous absorbent material shall be asbestos-free and may be used in the construction of the exhaust or silencing system only if suitable devices ensure that the fibrous material is kept in place for the whole time that the exhaust or silencing system is being used and the exhaust or silencing system meets the requirements of any one of paragraphs 1.1., 1.2.*,*1.3. or 1.4.:"

Insert a new paragraph 1.4. to read:

"1.4. Exhaust gases are not in contact with fibrous materials and fibrous materials are not under the influence of pressure variations."

*Annex 7,*

*Paragraph 2.5.,* add a note at the end to read:

"2.5. ASEP control range

…

*Note*: If the vehicle has more than one gear, the first gear shall not be used."

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)