|  |  |
| --- | --- |
|  | E/ECE/324/Rev.2/Add.112/Rev.3/Amend.5−E/ECE/TRANS/505/Rev.2/Add.112/Rev.3/Amend.5 |
|  |  | 22 February 2017 |

 Agreement

 Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

 Addendum 112 – Regulation No. 113

 Revision 3 - Amendment 5

Supplement 6 to the 01 series of amendments – Date of entry into force: 9 February 2017

 Uniform provisions concerning the approval of motor vehicle headlamps emitting a symmetrical passing-beam or a driving-beam or both and equipped with filament, gas-discharge light sources or LED modules

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2016/74.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 6.2.6.1.*, to be deleted.

*Paragraph 6.2.7.*, amend to read:

"6.2.7. Either one or two filament light sources (Classes A, B, C, D) or one gas discharge light source (Class E) or one or more LED module(s) (Classes A, B, C, D, E) are permitted for the principal passing-beam."

*Paragraph 6.3.2.,* amend to read:

"6.3.2. Irrespective of type of light source (LED module(s) or filament light source(s) or gas discharge light source) used to produce the passing-beam, several light sources either:

1. …
2. …
3. LED module(s) (Classes B, C, D, E) may be used for each individual driving-beam."

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)