|  |  |
| --- | --- |
|  | E/ECE/324/Rev.1/Add.18/Rev.7/Amend.5−E/ECE/TRANS/505/Rev.1/Add.18/Rev.7/Amend.5 |
|  |  | 27 March 2018 |

 Agreement

 Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

 Addendum 18 – UN Regulation No. 19

 Revision 7 - Amendment 5

Supplement 10 to the 04 series of amendments – Date of entry into force: 10 February 2018

 Uniform provisions concerning the approval of power-driven vehicle front fog lamps

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2017/76

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 5.6.,* amend to read:

"5.6. In the case of Class B, the front fog lamp shall onlybe equipped with one filament light source approved according to UN Regulation No. 37, even if the filament light source cannot be replaced. Any UN Regulation No. 37 approved filament light source may be usedprovidedthat;

(a) Its objective luminous flux does not exceed 2,000 lumens, and

(b) No restriction on the use is made in UN Regulation No. 37 and its series of amendments in force at the time of application for type approval.

5.6.1. Even if this filament light source cannot be replaced it shall comply with the requirements in paragraph 5.6. above."

*Paragraph 5.7.,* amend to read:

"5.7*.* In the case of Class F3, irrespective of whether the light sources can be replaced or not, the front fog lamp shall only be equipped with:

5.7.1. One or more light sources approved according to:

5.7.1.1. UN Regulation No. 37 and its series of amendments in force at the time of application for type approval, provided that no restriction on their use is made,

5.7.1.2. Or, UN Regulation No. 99 and its series of amendments in force at the time of application for type approval,

5.7.2. And/or, one or more LED modules where the requirements of Annex 12 to this Regulation shall apply; compliance with these requirements shall be tested."

1. \* Former titles of the Agreement:

 Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

 Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)