|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.1/Add.40/Rev.2/Amend.6−E/ECE/TRANS/505/Rev.1/Add.40/Rev.2/Amend.6 | |
|  |  | 2 November 2018 |

Agreement

Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

Addendum 40 – UN Regulation No. 41

Revision 2 - Amendment 6

Supplement 6 to the 04 series of amendments – Date of entry into force: 16 October 2018

Uniform provisions concerning the approval of motor cycles with regard to noise

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2018/6.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Annex 3*

*Paragraph 1.3.2.1.,* amend to read:

"1.3.2.1. General conditions

The vehicle shall be supplied as specified by the vehicle manufacturer.

Before the measurements are started, the vehicle shall be brought to its normal operating conditions.

If the motor cycle is fitted with fans with an automatic actuating mechanism, this system shall not be interfered with during the sound measurements. For motor cycles having more than one driven wheel, only the drive provided for normal road operation may be used. "

1. \* Former titles of the Agreement:

   Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

   Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)