|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.1/Add.47/Rev.12/Amend.6−E/ECE/TRANS/505/Rev.1/Add.47/Rev.12/Amend.6 | |
|  |  | 10 August 2018 |

Agreement

Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

Addendum 47 – UN Regulation No. 48

Revision 12 - Amendment 6

Supplement 10 to the 06 series of amendments – Date of entry into force: 19 July 2018

Uniform provisions concerning the approval of vehicles with regard to the installation of lighting and light-signalling devices

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2017/110 (as amended by paragraph 67 of the report ECE/TRANS/WP.29/1135).

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 5.11.1.3.* shall bedeleted.

*Paragraph 6.2.7.6.* shall be deleted.

*Paragraph 6.2.7.6.1.,* renumber as 6.2.7.6. and amend to read:

"6.2.7.6. The dipped-beam headlamps shall be switched ON and OFF automatically relative to the ambient light conditions (e.g. switch ON during night-time driving conditions, tunnels, etc.) according to the requirements of Annex 13."

*Paragraphs 6.2.7.6.2., 6.2.7.6.3. and its subparagraphs* shall be deleted.

*Paragraph 6.9.8.*, amend to read:

"6.9.8. Tell-tale

Circuit-closed tell-tale mandatory.

This tell-tale shall be non-flashing and shall not be required if the instrument panel lighting can only be switched ON simultaneously with the front position lamps.

However, a tell-tale indicating failure is mandatory if required by the component Regulation."

*Paragraph 6.10.8.*, amend to read:

"6.10.8. Tell-tale

Circuit-closed tell-tale mandatory. It shall be combined with that of the front position lamps.

However, a tell-tale indicating failure is mandatory if required by the component Regulation."

*Paragraph 6.19., footnote 14* shall be deleted.

*Paragraph 6.19.7.4.,* amend to read:

"6.19.7.4. The lamps referred to in paragraph 5.11. may be switched ON when the daytime running lamps are switched ON."

1. \* Former titles of the Agreement:

   Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

   Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)