|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.2/Add.105/Rev.2/Amend.7−E/ECE/TRANS/505/Rev.2/Add.105/Rev.2/Amend.7 | |
|  |  | 19 November 2019 |

Agreement

Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

Addendum 105 – UN Regulation No. 106

Revision 2 - Amendment 7

Supplement 17 to 00 series of amendments – Date of entry into force: 15 October 2019

Tyres for agricultural vehicles and their trailers

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2019/5.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

Supplement 17 to the original series of amendments to UN Regulation No. 106 (Tyres for agricultural vehicles and their trailers)

*Paragraph 1.*, amend to read:

"1. Scope

1.1. This UN Regulation applies to new pneumatic tyres\* designed primarily, but not only, for agricultural and forestry vehiclesin categories T, R and S1.

1.2. This UN Regulation does not apply to the following tyres:

1.2.1. Tyres identified by speed category symbols corresponding to speeds higher than 65 km/h (i.e. speed category symbols higher than "D").

1.2.2. Tyres designated primarily for other purposes, such as:

a) Earth-moving equipment;

b) Industrial and lift trucks."

*Paragraph 3.1.9.2. (former),* renumber as 3.1.10.1. and amend to read:

"3.1.10.1**.** The inscription 'I-3' for implement tyres with traction tread as identified in Annex 5, Tables 5 and 6."

*Annex 5,*

*Table 5, Note 3,* amend to read:

"3. Overall diameters (D) in column (\*) apply to tyres marked with classification code "I-3" – see paragraph 3.1.10.1. of this Regulation."

*Annex 5,*

*Table 6, Note 3,* amend to read:

"3. Overall diameters (D) in column (\*) apply to tyres marked with classification code "I-3" – see paragraph 3.1.10.1. of this Regulation."

*Annex 5,*

*Table 7 (3 of 4),* amend to read:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| *Tyre size*  *designation****5*** | *Theoretical*  *rim width*  *code (A1)* | *Nominal section*  *width (S1)*  *(mm)* | *Overall*  *diameter (D)*  *(mm)* | *Nominal rim*  *diameter (d)*  *(mm)* |
| ... | ... | ... | ... | ... |
| 36x16-17.5 | 10.5 | 406 | 914 | 445 |
| ... | ... | ... | ... | ... |

*Annex 7, Part E,* table, amend to read:

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *Speed (km/h)* | *Speed Category Symbol* | | | | |
| *A2* | *A8* | | *D* | |
| *Constant load* | *Cyclic applications (+)* | *Constant load* | *Cyclic applications (+)* |
| 5 | + 11 | + 45 | + 67 (1) | +67 | +92 (1) |
| 10 | 0 | + 25 | + 50 (2) | +44 | +73 (2) |
| 15 | - 21 | + 13 | + 34 | +30 | +54 |
| 20 | - 24 | + 9 | + 23 | +26 | +42 |
| 25 | - 28 | + 6 | + 11 | +22 | +28 |
| 30 | - 32 | + 4 | + 7 | +20 | +23 |
| 35 | - 33 | + 2 | + 3 | +18 | +19 |
| 40 | - 34 | 0 | 0 | +15 | +15 |
| 45 | - 35 | - 4 | - 4 | +12 | +12 |
| 50 | - 37 | - 9 | - 9 | +8 | +8 |
| 55 | - | - | - | +5 | +5 |
| 60 | - | - | - | +3 | +3 |
| 65 | - | - | - | 0 | 0 |
| 70 | - | - | - | -9 | -9 |

"

1. \* Former titles of the Agreement:

   Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

   Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)