|  |  |  |
| --- | --- | --- |
|  |  | ECE/TRANS/180/Add.6/Corr.2 |
|  |  | 30 January 2018 |

 Global registry

 Created on 18 November 2004, pursuant to Article 6 of the Agreement concerning the establishing of global technical regulations for wheeled vehicles, equipment and parts which can be fitted and/or be used on wheeled vehicles (ECE/TRANS/132 and Corr.1) done at Geneva on 25 June 1998

 Addendum 6: UN Global Technical Regulation No. 6

 Safety Glazing Materials for Motor Vehicles and Motor Vehicle Equipment

 Corrigendum 2

Established in the Global Registry on 15 November 2017

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_



**UNITED NATIONS**

*Part B, TEXT OF REGULATION*

*Paragraph 2., Application/Scope*, correct to read:

"2. APPLICATION/SCOPE

 This regulation applies to safety glazing intended for installation as windscreens or panes or as partitioning on Category 1 and 2 vehicles as defined in Special Resolution No. 1 (S.R.1) concerning the Common Definitions of Vehicle Categories, Masses and Dimensions, to the exclusion however of glazing for lighting and light-signalling devices and instrument panels, and of bullet resistant glazing. In the case of double windows, each pane is considered a separate item of glazing."

*Paragraph 6.3.2.3.*, correct to read:

"6.3.2.3. The point of impact shall be within 25 mm of the geometric centre of the test piece for a drop height less than or equal to 6 m, and within 50 mm of the centre of the test piece for a drop height greater than 6 m."