|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.2/Add.127/Amend.7/Corr.1−E/ECE/TRANS/505/Rev.2/Add.127/Amend.7/Corr.1 | |
|  |  | 17 October 2023 |

Agreement

Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

Addendum 127 – UN Regulation No. 128

Amendment 7 - Corrigendum 1

Corrigendum 1 to Supplement 7 to the original version of the Regulation – Date of entry into force:   
16 October 2018

Uniform provisions concerning the approval of light emitting diode (LED) light sources for use in approved lamp units on power-driven vehicles and their trailers

This document is meant purely as documentation tool. The authentic and legal binding texts is: ECE/TRANS/WP.29/2018/30.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Page 5,* *Annex 4, paragraph 5.5.,* amend to read:

“5.5. Colour variation

The colour variation is the maximum deviation of all colour points (given by the chromaticity coordinates x, y) at elevated temperatures T in the range as specified by paragraph 5.1., from the colour point (*x0*, *y0*) at:

1. 23° C, in case of an integrated heatsink:

;

(b) Tb, in case a temperature value Tb is defined:  
max{”

1. \* Former titles of the Agreement:

   Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

   Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)