UNITED

NATIONS

Distr.	GENERAL

TRANS/WP.29/617	15 May 1998

ENGLISH

Original:	ENGLISH

and FRENCH

INLAND TRANSPORT COMMITTEE

Working Party on the Construction of Vehicles

DRAFT SUPPLEMENT 8 TO THE 02 SERIES OF AMENDMENTS

TO REGULATION No. 19

(Front fog lamps)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its eighth session, following the recommendation by the Working Party at its one-hundred-and-fourteenth session. It is based on document TRANS/WP.29/1998/16, not amended (TRANS/WP.29/609, paras. 63 and 114).

GE.98-

Paragragh 2.2.1., amend to read:

"... specified; it shall be H1, H2, H3, H4, H7, H8, HB3, HB4, H27W/1, H27W/2, H10 or H11 filament lamp(s) as specified in Regulation No. 37;"

Paragraph 6.3., insert a new line to the existing table to read:

"H11	12	1000"

Annex 1, item 2, amend to read:

"2.	Front fog lamp using a filament lamp category H1, H2, H3, H4, H7, H8, HB3, HB4, H27W/1, H27W/2, H10, H11 2/......................."

___________________

2/	(note not modified)

____________