E/ECE/324

Add.10 / Rev.l / Amend.1

E/ECE/TRANS/505

5 April 1986

AGREEMENT

CONCERNING THE ADOPTION OF UNIFORM CONDITIONS OF APPROVAL

AND THE RECIPROCAL RECOGNITION OF APPROVAL

FOR MOTOR VEHICLE EQUIPMENT AND PARTS

done at Geneva on 20 March 1958

-----------------

Addendum 10: Regulation No. 11

Date of entry into force as an annex to the Agreement :

1 June 1969

Revision 1 - Amendment 1

Amendments * which entered into force on 20 April 1986

UNIFORM PROVISIONS CONCERNING THE APPROVAL OF VEHICLES

WITH REGARD TO DOOR LATCHES AND DOOR RETENTION COMPONENTS

__________

UNITED NATIONS

-----------------------

* Supplernent 1 to the 02 series of arnendrnents to this Regulatlon. This supplernent does not require any change in the approval number.

Paragraph 4.3, amend to read:

"Notice of approval or of extension or refusal of approval of a vehicle type pursuant to this Regulation shall be communicated to the Parties to the Agreement applying this Regulation, by means of a form conforming to the model in annex 1 to this Regulation."

Paragraph 5.1.2, should read:

"5.1.2	Each latch shall have a fully latched position, for hinged doors, an intermediate latched position shall also be provided."

Paragraph 5.1.3 (new), read:

"5.1.3	A sliding door which has no intermediate latched position shall automatically move away from the latch to a partially-opened position if the door has not reached the fully latched position, the partially-
opened position shall be readily apparent to occupants of the vehicle."

Paragraphs 5.1.3 and 5.1.4 (former), renumber as 5.1.4 and 5.1.5.

Title of paragraph 7, amend to reads

"MODIFICATION AND EXTENSION OF APPROVAL OF THE VEHICLE TYPE"

Add the following new paragraph:

"7.3	The competent authority issuing the extension of approval shall assign a series number to each communication form drawn up for such an extension."

Annex 3, paragraph 1.3, read:

"1.3	The means of attachment of the sample to the test fixture shall be the same as or be equivalent to the means used in normal production for attaching components to the vehicle."

Annex 1, to be replaced by the following:

"Annex 1

(M
aximum format: A4(210 x 297 mm))

2/

Communication concerning:	- the approval,

- the refusal of approval,

- the extension of approval,

- the approval withdrawn,

- the production definitely, discontinued.1/

of a vehicle type with regard to door latches and door retention components pursuant to Regulation No. 11

Approval No. . . . Extension No . . . .

1.	Trade name or mark of the motor vehicle:

2.	Vehicle type:

3.	Manufacturers name and address:

4.	Name and address of the manufacturer's representative (if applicable):

5.	Vehicle submitted for approval on:

6.	Technical Service responsible for conducting approval tests:

7.	Date of test report:

8.	Number of test report:

the type of vehicle with the number of doors

9.	Remarks:

(sedan 2 doors, 4 doors - station wagon 4 doors ...)

10.	Position of approval mark:

11.	Reason(s) of extension (if applicable):

12.	Approval granted/refused/extended/withdrawn. 1/ :

13.	Place:

14.	Date:

15.	Signature:

16.	The list of documents deposited at the administrative service which has granted approval is annexed to this communication and available upon request.

--------------

--------------

1/ Strike out what does not apply.

2/ Name of the administration."