**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods 16 September 2016**

**Joint Meeting of the RID Committee of Experts and the   
Working Party on the Transport of Dangerous Goods**

Geneva, 19–23 September 2016  
Item 4 of the provisional agenda

**Interpretation of RID/ADR/ADN**

Supporting information for ECE/TRANS/WP.15/AC.1/2016/32

Transmitted by the European Industrial Gases Association (EIGA)

To support ECE/TRANS/WP.15/AC.1/2016/32.6.2.15, the following photographs show examples of pressure drums as well as the location of where marks are applied. From these photographs, it will be seen that the marking of pressure drums is not always easy to accomplish due to the location of the where the marks are needed to be applied, for example on the inside face of the pressure drum shroud.

By having the information engraved on a ring that is affixed to the cylinder when the valve is installed means that the marks can be applied in conditions that assist in the clarity of the marks.



Examples of pressure drums



Example of a nameplate



Example of location of pressure drum nameplate



Example of location of a nameplate on the inner face of the pressure drum shroud