|  |  |  |
| --- | --- | --- |
|  |  | **INF.12** |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of the RID Committee of Experts and the**

**Working Party on the Transport of Dangerous Goods 5 September 2018**

Geneva, 17-21 September 2018

Item 5 (a) of the provisional agenda

**Proposals for amendments to RID/ADR/ADN:**

**pending issues**

 Information on the status of publication of standards adopted for RID/ADR 2019, not published before 1 June 2018

 Transmitted by the Government of France

1. As explained in detail in document ECE/TRANS/WP.15/AC.1/151/Add.1 under item 5 (a), the amendments concerning references to new standards or additives to referenced standards not published before 1 June 2018 were not included in the list of amendments for entry into force on 1 January 2019.

2. For ADR, these amendments were listed separately in Annexes III and IV of the report of WP.15 (ECE/TRANS/WP.15/242) as draft amendments adopted by WP.15 for entry into force as soon as possible following their publication. For RID, these amendments were also listed separately in Annex II of the report of the RID Committee of Experts’ standing working group (OTIF/RID/CE/GTP/2018-A).

3. The following annex reproduces the adopted amendments and specifies the date of publication of each of these standards.

 Annex

 Draft amendments relating to standards EN 14025:2018, EN 12972:2018, EN 13317:2018, EN 1440:2016 + A1:2018, EN 16728:2016 + A1:2018 and EN ISO 17871:2015 + A1:2018 for entry into force as soon as possible once the standards have been published.

**1. Draft amendments relating to standard EN 14025:2018**

**6.8.2.6.1** Amend the Table, under "For design and construction of tanks", as follows:

 – For standard "EN 14025:2013 + A1:2016", in column (4), replace "Until further notice" by:

"Between 1 January 2017 and 31 December 2020".

– After the standard "EN 14025:2013 + A1:2016", insert the following rows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN 14025:2018 | Tanks for the transport of dangerous goods – Metallic pressure tanks – Design and construction | 6.8.2.1 and 6.8.2.3 | Until further notice |  |

**ADR only**

**6.8.4 (d)** TT11 In the paragraph after the Table, replace "EN 14025:2013 + A1:2016" by: "EN 14025:2018”.

EN 14025:2018 published on 1/8/2018

**2. Draft amendments relating to standard EN 12972:2018**

**6.8.2.6.1** Amend the Table, under "For design and construction of tanks", as follows:

– After the new standard "EN 14025:2018", insert the following rows:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN 12972:2018 | Tanks for transport of dangerous goods – Testing, inspection and marking of metallic tanks | 6.8.2.3 | Mandatorily from 1 January 2021 |  |

**6.8.2.6.2** Amend the Table as follows:

– For standard "EN 12972:2007", in column (4), replace "Until further notice" by:

"Until 30 June 2019".

– After the standard "EN 12972:2007", insert the following row:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN 12972:2018 | Tanks for transport of dangerous goods – Testing, inspection and marking of metallic tanks | 6.8.2.46.8.3.4 | Mandatorily from 1 July 2019 |  |

EN 12972:2018 published on 4/7/2018

**3. Draft amendments relating to standard EN 13317:2018 (ADR only)**

In the Table, under "For equipment”, for standard “EN 13317:2002 + A1:2006”, in column (4), replace “Until further notice” by “Between 1 January 2009 and 31 December 2020”.

- After standard “EN 13317: 2002 + A1:2006”, add the following new standard:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN 13317:2018 | Tanks for transport of dangerous goods - Service equipment for tanks - Manhole cover assembly | 6.8.2.2 and 6.8.2.4.1 | Until further notice |  |

EN 13317:2018 published on 11/7/2018

**4. Draft amendments relating to standard EN 1440:2016 +A1:2018**

**6.2.4.2** Amend the Table as follows:

– For standard "EN 1440:2016 (except annex C)", in column (3), replace "Mandatorily from 1 January 2019" by: "Until 31 December 2020".

– After standard "EN 1440:2016 (except annex C)", add the following new standard:

|  |  |  |
| --- | --- | --- |
| EN 1440:2016 + A1:2018 (except Annex C) | LPG equipment and accessories – Transportable refillable traditional welded and brazed steel Liquefied Petroleum Gas (LPG) cylinders – Periodic inspection | Mandatorily from 1 January 2021 |

EN 1440:2016 + A1:2018 published on 13/6/2018

**5. Draft amendments relating to standard EN 16728:2016 +A1:2018**

**6.2.4.2** Amend the Table as follows:

– For standard "EN 16728:2016 (except clause 3.5, Annex F and Annex G)", in column (3), replace "Mandatorily from 1 January 2019" by: "Until 31 December 2020".

– After standard "EN 16728:2016 (except clause 3.5, Annex F and Annex G)" add the following new row:

|  |  |  |
| --- | --- | --- |
| EN 16728:2016 + A1:2018 | LPG equipment and accessories – Transportable refillable LPG cylinders other than traditional welded and brazed steel cylinders – Periodic inspection | Mandatorily from 1 January 2021 |

EN 16728:2016 + A1:2018 published on 13/6/2018

**6. Draft amendments relating to standard EN ISO 17871:2015 + A1:2018**

**6.2.4.1** Amend the Table, under "for closures", as follows:

– For standard "EN ISO 17871:2015", in column (4), replace "Until further notice" by: "Between 1 January 2017 and 31 December 2020".

– After standard "EN ISO 17871:2015", add the following new standard:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| EN ISO 17871:2015 + A1:2018 | Gas cylinders – Quick-release cylinder valves – Specification and type testing | 6.2.3.1, 6.2.3.3 and 6.2.3.4 | Until further notice |  |

EN ISO 17871:2015 + A1:2018 published on 1/8/2018

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_