|  |  |  |
| --- | --- | --- |
|  |  | **INF.18** |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of the RID Committee of Experts and the**

**Working Party on the Transport of Dangerous Goods 12 September 2018**

Geneva, 17-21 September 2018

Item 2 of the provisional agenda

**Tanks**

Inspections and tests of battery-wagons/battery-vehicles and MEGCs

Transmitted by the Government of France

1. RID/ADR 6.8.3.4.12 refers to 6.8.3.4.6 for the inspections and tests of battery-wagons/battery-vehicles and MEGCs the elements of which are tanks.

2. 6.8.3.4.6 defines the periodicity of the periodic inspections for tanks intended for the carriage of refrigerated gases, by derogation from the general rules of 6.8.2.4.2.

3. But refrigerated gases are not allowed to be carried in battery-wagons/battery-vehicles and MEGCs.

4. To avoid any misinterpretation we propose to replace in 6.8.3.4.12 the reference to 6.8.3.4.6 by the reference to 6.8.2.4.2.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_