|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2018/24 | |
| Description: _unlogo | **Economic and Social Council** | | Distr.: General  3 January 2018  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**174th session**

Geneva, 13-16 March 2018

Item 4.8.10 of the provisional agenda

**1958 Agreement:  
Consideration of draft amendments**

**to existing UN Regulations submitted by GRSG**

Proposal for Supplement 1 to the 03 series of amendments to UN Regulation No. 118 (Burning behaviour of materials)

**Submitted by the Working Party on General Safety Provisions**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on General Safety Provisions (GRSG) at its 113thsession (ECE/TRANS/WP.29/GRSG/92, para. 9). It is based on official document ECE/TRANS/WP.29/GRSG/2017/21. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their March 2018 sessions.

Supplement 1 to the 03 series of amendments to UN Regulation No. 118 (Burning behaviour of materials)

*Part II, paragraphs 6.1.1.2. to 6.2.2.*, amend to read:

"6.1.1.2. The intended use (seat upholstery, ceiling lining, insulation, etc.),

…

6.1.6. "Interior lining(s)" means material(s) that (together) constitute(s) the surface finish and substrate of a ceiling, wall or floor.

…

6.2.2. The following materials shall … this Regulation:

(a) … more than 500 mm above the seat cushion and on the ceiling of the vehicle,

(b) …"

*Annex 2*

*Paragraph 2.1.*, replace the words "in the roof" by "on the ceiling".

1. \* In accordance with the programme of work of the Inland Transport Committee for 2016–2017 (ECE/TRANS/254, para. 159 and ECE/TRANS/2016/28/Add.1, cluster 3.1), the World Forum will develop, harmonize and update UN regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)