|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2018/28 | |
| Description: _unlogo | **Economic and Social Council** | | Distr.: General  27 December 2017  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**174th session**

Geneva, 13-16 March 2018

Item 4.9.1 of the provisional agenda

**1958 Agreement:  
Consideration of draft amendments**

**to existing UN Regulations submitted by GRE**

Proposal for Supplement 29 to the 01 series of amendments to UN Regulation No. 6 (Direction indicators)

**Submitted by the Working Party on Lighting and Light-Signalling**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Lighting and Light-Signalling (GRE) at its seventy-eighth session (ECE/TRANS/WP.29/GRE/78, para. 13). It is based on Annex II to the report. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their March 2018 sessions.

Supplement 29 to the 01 series of amendments to UN Regulation No. 6 (Direction indicators)

*Paragraph 1.3.*,amend to read:

"1.3. "*Direction indicators of different types*" means lamps which differ in such essential respects as:

(a) the trade name or mark:

(i) lamps bearing the same trade name or mark but produced by different manufacturers shall be considered as being of different types;

(ii) lamps produced by the same manufacturer differing only by the trade name or mark shall be considered as being of the same type.

(b) the characteristics …"

1. \* In accordance with the programme of work of the Inland Transport Committee for 2016–2017 (ECE/TRANS/254, para. 159 and ECE/TRANS/2016/28/Add.1, cluster 3.1), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)