**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**108th session 13 November 2020**

Geneva, 10–13 November 2020

Item 6 of the provisional agenda

**Interpretation of ADR**

Interpretation of 8.5 S1 (6) - Security provisions for explosives and detonators

Note by the secretariat

In relation to the discussions on informal documents INF.9 and INF.14 the secretariat would like to raise the following points:

* Detonators classified 1.4B and 1.4S are included in S1 (6). It seems that UN Nos. 0512 and 0513 should have been added in the list when these new entries were adopted.

|  |  |  |  |
| --- | --- | --- | --- |
| 0512 | DETONATORS, ELECTRONIC programmable for blasting | 1 | 1.4B |
| 0513 | DETONATORS, ELECTRONIC programmable for blasting | 1 | 1.4S |

* UN Nos. 0512 and 0513 were added in the list in 1.10.4 so that the security provisions apply irrespective of the quantities transported. The same should probably apply to UN 0511. For the moment, the security provisions do not apply for quantities of detonators of UN 0511, classified 1.1B, under 20 kg.

These issues were probably overlooked during the process of harmonisation with the Model Regulations.

The secretariat will transmit them to the Joint Meeting for consideration.