|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2020/22 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  18 December 2019  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**180th session**

Geneva, 10–12 March 2020

Item 4.8.11 of the provisional agenda

**1958 Agreement:  
Consideration of draft amendments to existing   
UN Regulations submitted by GRSG**

Proposal for Supplement 04 to the 01 series of amendments to UN Regulation No. 121 (Identification of controls, tell-tales and indicators)

Submitted by the experts from the Working Party on General Safety[[1]](#footnote-1)\*

The text reproduced below was adopted by the Working Party on General Safety (GRSG) at its 117th session (ECE/TRANS/WP.29/GRSG/96, para. 56). It is based on ECE/TRANS/WP.29/GRSG/2019/17 as. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their March 2020 sessions.

Supplement 04 to the 01 series of amendments to UN Regulation No. 121 (Identification of controls, tell-tales and indicators)

*Table 1*, amend to read (adding the references to footnote 18):

"

| *No.* | *Column 1* | *Column 2* | *Column 3* | *Column 4* | *Column 5* |
| --- | --- | --- | --- | --- | --- |
|  | *Item* | *Symbol* ***2*** | *Function* | *Illumination* | *Colour* |
|  | … |  |  |  |  |
| 7. | Front fog lamps |  | Control | No |  |
|  |  | 1**, 18** | Tell-tale | Yes | Green |
| 8. | Rear fog lamp |  | Control | No |  |
|  |  | 1**, 18** | Tell-tale | Yes | Yellow |
|  | … |  |  |  |  |
| 17. | Windscreen defrosting and defogging system  (with separate operating control) | **18** | Control | Yes |  |
|  |  |  | Tell-tale | Yes | Yellow |
| 18. | Rear window defrosting and defogging system  (with separate operating control) | **18** | Control | Yes |  |
|  |  |  | Tell-tale | Yes | Yellow |
|  | … |  |  |  |  |
| 20. | Parking lamps | **18** | Control | No |  |
| Tell-tale | Yes | Green |
|  | … |  |  |  |  |
| 31. | Diesel pre-heat | **18** | Tell-tale | Yes | Yellow |
| 32. | Choke (cold starting device) | **18** | Control | No |  |
| Tell-tale |  | Yellow |
|  | … |  |  |  |  |

…

18 Symbol may be shown in other colours than specified in column 5 in order to convey different meanings according to the general colour coding as proposed in paragraph 5 of ISO 2575-2004.

… "

1. \* In accordance with the programme of work of the Inland Transport Committee for 2020 as outlined in proposed programme budget for 2020 (A/74/6 (part V sect. 20) para 20.37), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate.. [↑](#footnote-ref-1)