|  |  |
| --- | --- |
|  | E/ECE/TRANS/505/Rev.3/Add.152/Amend.1 |
|  |  | 2 July 2021 |

**Agreement**

 Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

 (Revision 3, including the amendments which entered into force on 14 September 2017)

**\_\_\_\_\_\_\_\_\_**

 **Addendum 152 – UN Regulation No. 153**

 Amendment 1

Supplement 1 to the original version of the Regulation – Date of entry into force: 9 June 2021

 Uniform provisions concerning the approval of vehicles with regard to fuel system integrity and safety of electric power train in the event of a rear-end collision

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2020/114.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 2.8.*, amend to read:

"2.8. "*Rechargeable Electrical Energy Storage System (REESS)*" means the rechargeable energy storage system that provides electric energy for electrical propulsion.

 A battery whose primary use is to supply power for starting the engine and/or lighting and/or other vehicle auxiliaries’ systems is not considered as a REESS.

 The REESS may include the necessary systems for physical support, thermal management, electronic controls and casing."

1. \* Former titles of the Agreement:

 Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

 Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)