|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.15/AC.2/2016/21/Corr.2 |
| _unlogo | **Economic and Social Council** | Distr.: General7 January 2016English only |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of Experts on the Regulations annexed to the
European Agreement concerning the International Carriage
of Dangerous Goods by Inland Waterways (ADN)
(ADN Safety Committee)**

**Twenty-eighth session**

Geneva, 25–29 January 2016
Item 6 of the provisional agenda

**Reports of informal working groups**

 Report of the tenth Meeting of the Informal Working Group on Explosion Protection on Tank Vessels

 Transmitted by the Central Commission for the Navigation of the Rhine[[1]](#footnote-2)

 Corrigendum 2

1. Page 3, paragraph 6, (a)

*In the first sentence, text in brackets, insert* “coupled unit” *after* “locks”.

2. Page 3, paragraph 6, (a), (i)

*Correct to read as follows:* “Surface temperatures ~~have to be below~~ shall not exceed 200 °C”.

3. Page 3, paragraph 6, (a), (ii)

*Correct to read as follows:* “Electrical equipment has to be of the type "limited explosion risk" (comparable to zone 2) as defined in ADN 1.2.1 whereas the surface temperature ~~is limited to~~ shall not exceed 200 °C.”

4. Page 3, paragraph 6, (a), (iii), second indent

*Insert* “at least” *after* “overpressure of”.

5. Page 4, paragraph 9

*Insert* “tank” *before* “vessels”.

6. Page 29, paragraph 5.4.3.4, second indent

*Insert* “installations and” *before “*equipment*”.*

7. Page 33, paragraph 7.2.3.51.4 new

*In the first sentence insert* “and non-electrical” *after* “electrical”.

8. Page 35, paragraph 7.2.4.22.2

*Correct the first sentence to read as follows: “*Opening of sampling outlets ~~and ullage openings and opening of the housing of the flame arrester~~ shall not be permitted except for the purpose of taking samples inspecting or cleaning empty cargo tanks.”

9. Page 39, paragraph 8.1.7.2 new

*In the headline, replace “*9.1.0.51” *by “*9.3.1.51, 9.3.2.51 or 9.3.3.51”.

*In the first sentence, insert “*installations” *after “*Such”.

*In the first sentence, replace “*9.3.1.50, 9.3.2.50 or 9.3.3.50” *by “*8.1.3.2”.

10. Page 44, paragraph 9.1.0.52.1

*In the first sentence, insert* “installation and” *after “*Electrical”.

*Replace “*9.1.0.12.4” *by “*9.1.0.12.3”.

11. Page 45, paragraph 9.1.0.53.5 new

*Replace* “IEC-60 245-4:1994” *by* “IEC-60 245-4:2011”.

1. Distributed in German by the Central Commission for the Navigation of the Rhine under the symbol CCNR-ZKR/ADN/WP.15/AC.2/2016/21/Corr.2. [↑](#footnote-ref-2)