|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2019/107 |
| _unlogo | **Economic and Social Council** | Distr.: General28 August 2019Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**179th session**

Geneva, 12-14 November 2019

Item 4.8.5 of the provisional agenda

**1958 Agreement:
consideration of draft amendments to existing
UN Regulations submitted by GRSP**

 Proposal for Supplement 5 the 03 series of amendments to UN Regulation No. 29 (Cabs of commercial vehicles)

 Submitted by the experts from the Working Party on Passive Safety[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Passive Safety (GRSP) at its sixty-fifth session (ECE/TRANS/WP.29/GRSP/65, para. 24). It is based on ECE/TRANS/WP.29/GRSP/2019/2. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their November 2019 sessions.

 Supplement 5 the 03 series of amendments to UN Regulation No. 29 (Cabs of commercial vehicles)

*Annex 3*, *paragraph 7.4.4.1.*, amend to read:

"7.4.4.1. It is parallel to the x-y plane of the chassis; during the application of the load, the loading device may deviate by not more than 5° in z-direction from the parallel plane to the x-y plane of the chassis in each direction."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2018–2019 (ECE/TRANS/274, para. 123 and ECE/TRANS/2018/21/Add.1, Cluster 3.1), the World Forum will develop, harmonize and update UN regulations to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)