UNITED

NATIONS

Distr.	GENERAL

TRANS/WP.29/636	2 June 1998

ENGLISH

Original:	ENGLISH

and FRENCH

INLAND TRANSPORT COMMITTEE

Working Party on the Construction of Vehicles

CORRIGENDUM 2 TO SUPPLEMENT 2 TO THE 01 SERIES OF AMENDMENTS

TO REGULATION No. 90

(Replacement brake linings)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its eighth session, following the recommendation by the Working Party at its one-hundred-and-fourteenth session. It is based on document TRANS/WP.29/1998/8, not amended (TRANS/WP.29/609, paras. 83 and 132).

Annex 4, paragraph 2.2.1.5.4., correct the words "by vehicle mass" to read "by one-half of the vehicle mass".

Annex 8, paragraph 3.2.2., correct to read:

"... a number of X braking intervals of 5 seconds brake applied followed by 10 seconds brake released."

GE.98-