UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/669
16 April 1999

ENGLISH ONLY

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

Working Party on the Construction of Vehicles

CORRIGENDUM 3 TO REVISION 1 OF

REGULATION No. 36

(Public service vehicles)

Note:	The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its eleventh session, following the recommendation by the Working Party at its one-hundred-and- seventeenth session. It is based on document TRANS/WP.29/1999/12, not amended (TRANS/WP.29/663, para. 118).

_________

GE.99-

Annex 3, figure 1, the table below the figure correct to read:

Dimension A (cm)	Alternative (cm)
Class I	110	110
Class II	95	110
Class III	85	110

____________