UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/685

23 July 1999

ENGLISH

Original: ENGLISH and

FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

Working Party on the Construction of Vehicles

CORRIGENDUM 1 TO SUPPLEMENT 1 TO THE 03 SERIES OF

AMENDMENTS TO REGULATION No. 83

(Emissions of M1 and N1 categories of vehicles)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its twelfth session, following the recommendation by the Working Party at its one-hundred-and-eighteenth session. It is based on document TRANS/WP.29/1999/20, not amended (TRANS/WP.29/680, para. 127).

__________

GE.99-

Paragraph 1.1., add at the end:

"........ four wheels.

It does not apply to vehicles with an unladen mass of less than 400 kg, or to vehicles with a design speed not exceeding 50 km/h.

At the request of the manufacturer, type approval according to this Regulation may be extended from M1 or N1 category vehicles equipped with compression-ignition engines which have already been type approved,

to M2 or N2 category vehicles having a reference mass not exceeding 2,840 kg and meeting the conditions of paragraph 7. (extension of approval)."

___________