|  |
| --- |
| **UN/SCETDG/49/INF.63** |
| **Committee of Experts on the Transport of Dangerous Goodsand on the Globally Harmonized System of Classificationand Labelling of Chemicals****Sub-Committee of Experts on the Transport of Dangerous Goods 29 June 2016****Forty-ninth session**Geneva, 27 June – 6 July 2016Item 4 (d) of the provisional agenda**Electric storage systems: miscellaneous** |

 UN Informal Meeting on Lithium Batteries – 2015-2016 3rd Session, 30 March – 1 April 2016 – Bordeaux, France

 Text proposed by the Informal working group for parag 2.9.4.f (complement of proposal 1 in Working paper 33)

* (f) lithium batteries, containing both primary lithium metal cells and rechargeable lithium ion cells, that are not designed to be externally charged (see special provision 387) shall meet the following conditions:

~~(a) It is not designed to be externally charged;~~

(b) The rechargeable lithium ion cells can only be charged from the primary lithium metal cells;

(c) Overcharge of the rechargeable lithium ion cells is precluded by design;

(d) The battery has been tested as a lithium primary battery;

(e) Component cells of the battery shall be of a type proved to meet the respective testing requirements of the Manual of Tests and Criteria, part III, sub-section 38.3.