|  |  |  |
| --- | --- | --- |
|  | **INF. 2** | |
| **Economic Commission for Europe**  **ADN Administrative Committee**  **Seventeenth session**  Geneva, 26 August 2016 Agenda item 3 (b) **Matters relating to the implementation of ADN:**  Special authorizations, derogations and equivalents | | **18 August 2016** |

Special authorisation, derogation and equivalents

Special Authorisation delivered to Monument Chemical Bvba – B – 9130 KALLO

Submitted by the Government of Belgium

I. Introduction

1. May 2016, the Belgian authority (Flemish Government) received a written request from Monument Chemicals bvba to evaluate if there was a possibility to transport the substance UN 1148 DIACETONE ALCOHOL in tank vessels from Monument Chemicals bvba – Ketenislaan 3 – Haven 1972 – 9130 Kallo, Belgium to LBC Rotterdam BV – Haven 4035 – Oude Maasweg 4 – 3197 KJ BOTLEK, The Netherlands. Monument Chemical mentioned that the substance could be found in part 3, table A of the annexes ADN, but not in table C.

II. Notification

2. Referring to ADN 1.5.2.1 and in accordance with paragraph 2 of article 7 of ADN, a competent authority have the right to issue a special authorization to a carrier for the international carriage in tank vessels of dangerous substances of which in tank vessels is not authorized under the ADN regulations.

3. Keeping in mind that the carriage shall take place not only on the territory of Belgium but also on the territory of a Member State (the Netherlands), the Member State was immediately informed about this request. All the necessary information about the product, transportation mode, etc. was transferred to the Netherlands.

4. August 2016, the government of the Netherlands informed the government of Belgium that had no objection and that they should allow the carriage of UN 1148 DIACETONE ALCOHOL on their territory.

5. A special authorisation was made with a validity from 01/09/2016 to 01/09/2018 and can be found in annex to this document.

6. As stated in ADN 1.5.2.2.2 the competent authority would like to inform the Administrative Committee of the existence of this special authorisation.

III. Proposal

7. The government of Belgium will propose the Administrative Committee to evaluate if the substance is to be included in the list of substances (table C) authorized of carriage in tank vessels. If positive, table A should also be adapted with a letter “T” in column 8.

Attachments

8. Please find attached:

The Special Authorisation

The Safety Data Sheet for UN1148 DIACETONE ALCOHOL

Annex I

Special authorization no.: ADN-001-2016

Pursuant to Article 5 – Royal Decree of 31 July 2009

Having regard to the Royal Decree of 31 July 2009 on the carriage of dangerous goods by inland waterways (ADN), amended by the Royal Decree of 4 July 2011 amending the regulations governing the carriage of dangerous goods by inland waterways to scientific and technical progress, the carriage of the materials mentioned in this Special Authorization by tank vessels is authorized subject to the conditions laid down therein.

Special Authorization ADN-001-2016 applies to **MONUMENT CHEMICAL, Port 1972 – Ketenislaan 3, B-9130 Kallo (Kieldrecht)** for the carriage in tank vessels from Belgium (Monument Chemical bvba – Ketenislaan 3 – Port 1972 – 9130 Kallo) to the Netherlands (LBC Rotterdam BV – Oude Maasweg 4 – Port 4035 – 3197 KJ Botlek) of the following product:

**UN 1148 DIACETONE ALCOHOL, 3, III**

This Special Authorization AND-001-2016 is valid, unless previously revoked, until 01/09/2018 inclusive.

Ostend, 01/09/2016 Head of unit

Didier Delaere, Ing.

Annex II

Safety Data Sheet for UN1148 DIACETONE ALCOHOL

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| (1) | (2) | (3a) | (3b) | (4) | (5) | (6) | (7a) | (7b) | (8) | (9) | (10) | (11) | (12) | (13) |
|  | 3.1.2 | 2.2 | 2.2 | 2.1.1.3 | 5.2.2 | 3.3 | 3.4 | 3.5.1.2 | 3.2.1 | 8.1.5 | 7.1.6 | 7.1.6 | 7.1.5 | 3.2.1 |
| UN no./substance no. | Name and description | Class | Classification code | Packing group | Labels | Special provisions | Limited quantity | Excepted quantity | Carriage permitted | Equipment required | Ventilation | Measures to be taken during loading, unloading and carriage | Number of blue lights | Extra requirements or remarks |
| 1148 | DIACETONE ALCOHOL | 3 | F1 | III | 3 | --- | 5I | E1 | --- | PP,A,EX | VE01 |  | 0 |  |

**The following requirements apply to the transport:**

1. The transport must take place with a classified tank vessel:

a. type N (condition of cargo tank / type of cargo tank) 3.2 / 2.2 / 2.3

b. type C

2. The transport must take place according to the minimum requirements stated in the request.