|  |  |  |
| --- | --- | --- |
|  |  | **INF.14**  |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**101st session 31 October 2016**

Geneva, 8–11 November 2016

Item 5(b) of the provisional agenda

**Proposals for amendments to annexes A and B of ADR:**

**miscellaneous proposals**

 8.1.5.2: EN 471 and warning vest

 Transmitted by the Government of Finland

**Reference to EN 471**

1. ADR 8.1.5.2 includes requirement on a warning vest for each member of the vehicle crew:

 “- A warning vest (e.g. as described in the EN 471:2003 + A1:2007 standard);”

2. We have been informed that EN 471 has been repealed. The corresponding standard is EN ISO 20471 Highly visibility clothing. Test methods and requirements.

3. Working Party may wish to update the reference to the relevant standard in 8.1.5.2.

**Vest or jacket**

4. In EN ISO 20471, it is mentioned that

- “garments covering only the torso” are for example vests and tabards; and

- “garments covering torso and arm” are for example jackets, shirts, coats and t-shirts

In ADR, term “warning vest” is used. We have been asked whether this is meant to limit the requirement to garments covering only the torso and if jackets are allowed.

5. To our understanding, the meaning of the requirement is to have appropriate warning clothing. It seems that appropriate warning clothing could be a garment covering torso and arms i.e. a jacket or a coat.

6. Finland would like to ask the opinion of the Working Party on this matter.