|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2018/77 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  9 April 2018  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**175th session**

Geneva, 19-22 June 2018

Item 4.6.8 of the provisional agenda

**1958 Agreement:  
Consideration of draft amendments**

**to existing UN Regulations submitted by GRSP**

Proposal for Supplement 1 to the 01 series of amendments to UN Regulation No. 137 (Frontal impact with focus on restraint systems)

**Submitted by the Working Party on Passive Safety**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Passive Safety (GRSP) at its sixty-second session (ECE/TRANS/WP.29/GRSP/62, para. 38). It is based on GRSP-62-05 as reproduced in Annex VIII to the report. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their June 2018 sessions.

Supplement 1 to the 01 series of amendments to UN Regulation No. 137 (Frontal impact with focus on restraint systems)

*Annex 3*

*Paragraph 5.2.4.1.*, amend to read:

"5.2.4.1. The axial compressive force is measured with a CFC of 600."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2018–2019 (ECE/TRANS/274, para. 123 and ECE/TRANS/2018/21/Add.1, cluster 3.1), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)