|  |  |
| --- | --- |
| Submitted by the experts from ETRTO | Informal document **GRRF-86-31**  86th GRRF, 12-16 February 2018  Agenda item 7(e) |

Proposal for amendments to ECE/TRANS/WP.29/GRRF/2018/6 and ECE/TRANS/WP.29/GRRF/2018/12.

I. Proposal

*Add a new paragraph 2.47. to read:*

"2.47. SS differentiates tyres for off-highway vehicles such as mini and skid-steer loaders from other tyres which use similar size designations, but may use different rim bead seat configurations."

II. Justification

Following the addition of Paragraph 2.18.12.1. to UN R106 (doc. ECE/TRANS/WP.29/GRRF/2018/6) the inscription “SS” was added but the definition was not provided: this informal document proposes the addition of a paragraph at the end of the Clause to provide such definition.