|  |  |  |
| --- | --- | --- |
|  | **INF.28** | |
| **Economic Commission for Europe**  Inland Transport Committee  **Working Party on the Transport of Dangerous Goods**  **Joint Meeting of Experts on the Regulations annexed to the European Agreement concerning the International Carriage of Dangerous Goods by Inland Waterways (ADN) (ADN Safety Committee)**  **Thirty-sixth session**  Geneva, 27-31 January 2020  Item 3 (c) of the provisional agenda  **Implementation of the European Agreement concerning the International Carriage of Dangerous Goods by Inland Waterways (ADN): interpretation of the Regulations annexed to AND** | | 29 January 2020 German |

Muster des Zulassungszeugnisses in ADN 8.6.1.3

Übermittelt von EBU/ESO

Ziffer 10 des Zulassungszeugnisses lautet:

10. Autonome Schutzsysteme

● Explosionsgruppe / Untergruppe der Explosionsgruppe II B: …..

Engl. ● Explosion group/subgroup of explosion group II B: ….....

EBU / ESO schlägt vor, die Worte “der Explosionsgruppe II B / of explosion group II B” zu streichen, so dass der betreffende Punkt lautet:

10. Autonome Schutzsysteme

● Explosionsgruppe / Untergruppe: ………

Engl. ● Explosion group/subgroup: ……..

Die vorgeschlagene Darstellung ist klarer. Im ADN wird ansonsten immer nur von Explosionsgruppe / Untergruppe gesprochen.