|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2020/50 |
| _unlogo | **Economic and Social Council** | Distr.: General2 April 2020Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**181st session**

Geneva, 23-25 June 2020

Item 4.6.1 of the provisional agenda

**1958 Agreement:
Consideration of draft amendments to existing
UN Regulations submitted by GRSP**

 Proposal for Supplement 1 to the 09 series of amendments to UN Regulation No. 14 (Safety-belt anchorages)

 Submitted by the Working Party on Passive Safety [[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Passive Safety (GRSP) at its sixty-fifth session (ECE/TRANS/WP.29/GRSP/66, para. 16). It is based on GRSP-66-16, as reproduced in Annex II to the report. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee (AC.1) for consideration at their June 2020 sessions.

*Annex 6, key to symbols 3*: amendto read:

"Annex 6

…

3: Two lower anchorages and one upper anchorage which allow the installation of a three-point safety-belt type A, or of safety-belts types Ar, Ar4m or Ar4Nm, where required by UN Regulation No. 16, Annex 16."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2020 as outlined in proposed programme budget for 2020 (A/74/6 (part V sect. 20) para 20.37), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)