|  |  |
| --- | --- |
|  | E/ECE/324/Rev.1/Add.73/Rev.2/Amend.3−E/ECE/TRANS/505/Rev.1/Add.73/Rev.2/Amend.3 |
|  |  | 11 July 2016 |

 Agreement

 Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

 Addendum 73 – Regulation No. 74

 Revision 2 – Amendment 3

Supplement 9 to the 01 series of amendments\*\* – Date of entry into force: 18 June 2016

 Uniform provisions concerning the approval of category L1 vehicles with regard to the installation of lighting and light-signalling devices

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2015/79.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 5.13.*, amend to read (footnote 3 remains unchanged):

"5.13. Colours of the lights3

The colours of the lights referred to in this Regulation shall be as follows:

Driving beam headlamp: white

Passing beam headlamp: white

Front position lamp: white

Front retro-reflector, non-triangular: white

Side retro-reflector, non-triangular: amber at the front

 amber or red at the rear

Pedal retro-reflector: amber

Rear retro-reflector, non-triangular: red

Direction-indicator lamp: amber

Stop lamp: red

Rear position lamp: red

Rear-registration plate lamp: white

Vehicle-hazard warning signal: amber"

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958.

 \*\* On the request of Office of Legal Affairs, this document is issued as Supplement 9 to the 01 series of amendments to Regulation No. 74 replacing the proposal for a Corrigendum1 to Supplement 8 to the 01 series as approved by WP.29. at its 167th session. [↑](#footnote-ref-2)