|  |  |
| --- | --- |
|  | E/ECE/324/Rev.1/Add.44/Rev.2/Amend.4−E/ECE/TRANS/505/Rev.1/Add.44/Rev.2/Amend.4 |
|  |  | 26 July 2017 |

 Agreement

 Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

 Addendum 44 – Regulation No. 45

 Revision 2 – Amendment 4

Supplement 10 to the 01 series of amendments – Date of entry into force: 22 June 2017

 Uniform provisions concerning the approval of headlamp cleaners, and of power-driven vehicles with regard to headlamp cleaners

This document is meant purely as documentation tool. The authentic and legal binding texts is: ECE/TRANS/WP.29/2016/77.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Annex 4,*

*Paragraph 2.1.2.,*amend to read:

"2.1.2. For headlamp with the outside lens in plastic material:

The mixture of water and polluting agent to be applied to the headlamp shall be composed of:

(a) 9 parts by weight of silica sand with a particle size of 0-100 μm;

(b) 1 part by weight of vegetal carbon dust produced from beech wood with a particle size of 0-100 μm;

(c) 0.2 part by weight of NaCMC1;

(d) 5 parts by weight of sodium chloride (pure at 99 per cent);

(e) 13 parts by weight of distilled water with a conductivity of ≤ 1 mS/m;

(f) 2 ± 1 drops of surfactant.2"

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)