|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.1/Add.45/Rev.6/Amend.2−E/ECE/TRANS/505/Rev.1/Add.45/Rev.6/Amend.2 | |
|  |  | 26 July 2017 |

Agreement

Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

Addendum 45 – Regulation No. 46

Revision 6 - Amendment 2

Supplement 4 to the 04 series of amendments – Date of entry into force: 22 June 2017

Uniform provisions concerning the approval of devices for indirect vision and of motor vehicles with regard to the installation of these devices

This document is meant purely as documentation tool. The authentic and legal binding texts is: ECE/TRANS/WP.29/2016/89.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 6.2.1.2.,* amend to read:

"6.2.1.2. If a device for indirect vision …… the total process of scanning, rendering and reset to its initial position together shall not take more than 200 milliseconds at room temperature of 22 °C ± 5 °C."

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)