|  |  |
| --- | --- |
| 6 | E/ECE/324/Rev.2/Add.120/Rev.1/Amend.6−E/ECE/TRANS/505/Rev.2/Add.120/Rev.1/Amend.6 |
|  |  | 26 July 2017 |

 Agreement

 Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

 Addendum 120 — Regulation No. 121

 Revision 1 — Amendment 6

Supplement 9 to the original version of the Regulation — Date of entry into force: 22 June 2017

 Uniform provisions concerning the approval of vehicles with regard to the location and identification of hand controls, tell-tales and indicators

This document is meant purely as documentation tool. The authentic and legal binding texts is: ECE/TRANS/WP.29/2016/96.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*In Table 1, lines Nos. 2. and 19., add a reference to existing note 18*, to read:

"Table 1

**Symbols, their illumination and colours**

| *No.* | *Column 1* | *Column 2* | *Column 3* | *Column 4* | *Column 5* |
| --- | --- | --- | --- | --- | --- |
|  | *Item* | *Symbol* ***2*** | *Function* | *Illumination* | *Colour* |
| *…* | *…* | *…* | *…* | *…* | *…* |
| 2. | Headlamp passing beams | Low beam 1, 6, 13, 18 | Control | No |  |
| Tell-tale | Yes | Green |
| *…* | … | … | … | … | … |
| 19. | Position, side marker, and/or end-outline marker lamps |  1, 6, 18 | Control | No |  |
| Tell-tale 12 | Yes 6 | Green |
| *…* | *…* | *…* | *…* | *…* | *…* |

…"

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)