|  |  |
| --- | --- |
|  | E/ECE/324/Rev.2/Add.133/Amend.2−E/ECE/TRANS/505/Rev.2/Add.133/Amend.2 |
|  |  | 22 February 2017 |

 Agreement

 Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

 Addendum 133 – Regulation No. 134

 Amendment 2

Supplement 02 to the original version of the Regulation – Date of entry into force:
9 February 2017

 Uniform provisions concerning the approval of motor vehicles and their components with regard to the safety-related performance of Hydrogen-Fuelled Vehicles (HFCV)

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2016/39.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Annex 3,*

*Paragraph 3.4.*, amend to read:

"3.4. Chemical exposure and ambient-temperature pressure cycling test

 …

Pressure cycling is performed to the specified target pressures according to paragraph 2.2. of this Annex at 20 (±5) °C for the specified numbers of cycles. The glass wool pads are removed and the container surface is rinsed with water the final 10 cycles to specified final target pressure are conducted."

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)