|  |  |
| --- | --- |
|  | E/ECE/324/Rev.2/Add.120/Rev.2/Amend.3−E/ECE/TRANS/505/Rev.2/Add.120/Rev.2/Amend.3 |
|  |  | 2 November 2018 |

 Agreement

 Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

 Addendum 120 – UN Regulation No. 121

 Revision 2 - Amendment 3

Supplement 3 to the 01 series of amendments — Date of entry into force: 16 October 2018

 Uniform provisions concerning the approval of vehicles with regard to the location and identification of hand controls, tell-tales and indicators

This document is meant purely as documentation tool. The authentic and legal binding texts is: ECE/TRANS/WP.29/2018/26.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Table 1, Symbol No. 1,* amend to read(adding a reference to existing footnote 18):

"

| *No.* | *Column 1* | *Column 2* | *Column 3* | *Column 4* | *Column 5* |
| --- | --- | --- | --- | --- | --- |
|  | *Item* | *Symbol* ***2*** | *Function* | *Illumination* | *Colour* |
| 1. | Master lighting switchTell-tale may not act as the tell-tale for the position (side) lamps |  1, 18 | Control | No |  |
| Tell-tale 12 | Yes  | Green |
| … | … | … | … | … | … |

"

1. \* Former titles of the Agreement:

 Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

 Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)