|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.1/Add.73/Rev.2/Amend.6−E/ECE/TRANS/505/Rev.1/Add.73/Rev.2/Amend.6 | |
|  |  | 1 July 2020 |

Agreement

Concerning the Adoption of Harmonized Technical United Nations Regulations for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these United Nations Regulations[[1]](#footnote-2)\*

(Revision 3, including the amendments which entered into force on 14 September 2017)

\_\_\_\_\_\_\_\_\_

Addendum 73 – UN Regulation No. 74

Revision 2 - Amendment 6

Supplement 12 to 01 series of amendments – Date of entry into force: 29 May 2020

Uniform provisions concerning the approval of category L1 vehicles with regard to the installation of lighting and light-signalling devices

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2019/87.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 3.2.5.,* amend to read:

"3.2.5. A statement of the method used for the definition of the apparent surface (see paragraph 2.6.);"

*Insert a new paragraph 3.2.6.,* to read:

"3.2.6. At the discretion of the manufacturer, a statement indicating whether lamps approved for and equipped with LED substitute light sources are allowed to be installed on the vehicle or not and, if this is allowed, which lamps."

*Insert a new paragraph 5.20*., to read:

"5.20. The use of lamps approved for and equipped with LED substitute light source(s), is allowed exclusively in the case where the statement indicated in paragraph 3.2.6. is present and positive.

To verify that this statement is respected, both at the type approval and in the conformity of production verification, the presence of the marking on the lamps related to the use of LED substitute light source(s) shall be checked."

*Annex 1*

*Insert a new item 5.12. and a new footnote 5,* to read:

"5.12. Lamps approved for and equipped with LED substitute light source(s) are allowed to be installed on this vehicle type: yes/no2, 5

5 If yes, list the applicable lamps."

1. \* Former titles of the Agreement:

   Agreement concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958 (original version);

   Agreement concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions, done at Geneva on 5 October 1995 (Revision 2). [↑](#footnote-ref-2)